Installation of Monitor for Freelander 2

2
1

3

卸下螺钉

卸下螺钉

1

2

3

3

3

1、A.Unclench the cover of speaker.
B.And then take out the plastic sheet. C.Finally, get out of screws.

、A.Cover the head of gearlever firstly;

2

B.Hold the central control panel to take out the frame.

3、Pull out the central control panel as the picture show

5

4

、Take out the screws on the left of CD changer and air conditioner.

、Take out the screws on the right of CD changer and air conditioner.

6、Pull out the CD changer & air conditioner & power wiring harness as the picture shows.

7、Take out the panel of  air conditioner as
shown on the picture.	8、Unclench and pull up the cover of gear lever    9、Take out screw highlighted with red frame

10、Firstly, Take out the cover of as well as its screws ;
Secondly, take out the big frame shown on the picture and pull out the wiring harness.

11、Connect the power wiring harness to the original power out wiring harness as shown on pictures.

12、Put the wiring harness of monitor through the bottom and then fix the gear lever back

接上手刹车控制线

将后排中间盖按原厂固定

13

、Connect with the wiring harness of
hand brake	14、Fix the cover as the car  original design

1		Connect  the AUX OUT wiring harness as picture show

撬开喇叭网罩

GPS天线

注意GPS天线摆放位置

16、Unclench the right side grid cover	17、Fix the antenna of GPS on the foam

18、Take out the cover of air outlet of air conditioner;
Put the antenna of GPS in the central control station
Fix the grid cover of speaker back.

装喇叭弹片

19

the

、Fix the secure device of speaker as picture show

、Fix speaker into the hole on the centrol control

20

sta

tion.	21、Screw and fix the speaker

AV input cable

22、Firstly, Connect the wiring harness

Connector of

connector of

5

、

of original CD changer & air onditioner.
Secondly, fix & screw the CD changer

23、Insert the relativtive all these wiring
harnesses into the monitor	24、Connect the AV cable

connect the original cable of car

25、Take down the protection film. Fix the monitor as the picture shows

26、Fix &screw the securing device of monitor.	、Connect the flat cable to key control box corretly

2

7

and then fix the key control box.

2

9

28、Close the unclenched cover of speaker to finish the assemble of monitor

、If you need take out the key control box, please press the box gently from up to down.

Installation of Camera (CCD)

钻孔Φ10MM

1、Bore a hole in the bumper, whose diameter is Φ10MM

2、Dismount the right rear taillight as the picture shows

、Fix the Camera on bumper and connect with camera connecting wiring harness

3

车后尾灯黑兰线与主机黑线

绿白线与主机兰线连

黑兰线与主机黑线连

车后尾灯绿白线与主机兰线

4、Fix the filter box on the right rear taillight & connect with connecting wiring harness

、Note: Connect the black cable of rear taillight with the black cable of monitor.

5

Connect the green & white cable of rear taillight with the blue one of monitor.
Enwrap the cable "B+" with tape from touching with others

6、Fix the CCD cable on the socket of real taillight and enwrap the cable with electrical tape as shown on the former step

7、Fix the connecting wiring harness on rear box of car as the picture shows

8

、Put through the wiring cable from the right side of rear box as the picture shows

9、The picture of camera connecting wiring harness

1

0

、Put the camera connecting cable through along the right door as the picture shows

11、The position to fix the camera connecting cable

12、Put the cable through the assistant driver seat  as the picture shows

1

3

、The parking sensor is assembled then

The scketch to connect all accessories

As the step 15：insert the AUX OUT wiring harness

Step 19-21, speaker of central control station

The audio wiring harness

speaker

Step 23:connect antenna of GPS
GPS Antenna

Step 11: insert power wiring harness
Power wiring harness

Step23-26：Fix the monitor

Monitor

Step 5-6: fix the camera wiring harness Camera connecting wiring harness

Step 13：Connect the hand brake cable

Step 25: fix Securing device of monitor

Step 23:Insert the socket of wire harness of monitor

Step 1-4:assemble of camera

Camera

Plug of wiring harness of monitor